OCCUPANCY SENSOR INSPECTION

id092200801100

1. Turn the ignition switch to LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable and wait 1 min or more.

4. Remove the passenger-side seat. (See SEAT REMOVAL/INSTALLATION.)

5. Disconnect the occupancy sensor connector.

amxzzw00001754

6. Verify that the continuity between the occupancy sensor terminals is as indicated in the table.

amxzzw00001755

  • If not as indicated in the table, replace the occupancy sensor.

amxzzw00001756