PASSENGER AIR BAG DEACTIVATION (PAD) INDICATOR REMOVAL/INSTALLATION

id081000800400

1. Turn the ignition switch to the LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the following parts:

  (1) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (2) Center panel unit (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

  (3) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (4) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

5. Remove the screws.

amxzzw00001782

6. Disconnect the connector.

7. Remove the passenger air bag deactivation (PAD) indicator.

8. Install in the reverse order of removal.