HINGE PILLAR (OUTER) REMOVAL [PANEL REPLACEMENT]

id098008613500

1. Drill the 2 locations indicated by (A) from the interior.

2. Remove the hinge pillar (outer).

3. Remove the spot weld sealer using a disc grinder.

d5u0980b074

4. Remove the cowl side panel.

5. Remove the spot weld sealer using a disc grinder.

d5u0980b075

6. Remove the front pillar reinforcement.

d5u0980b076

7. Remove the front pillar (inner).

d5u0980b077