OIL FILTER CONSTRUCTION [L8, LF]

id0111c6100800

• The oil filter component is installed on the left surface (vehicle left) of the cylinder block.
• An aluminum oil filter adapter has been adopted for weight reduction. The oil pressure switch and oil cooler are installed on the oil filter adapter.
• The oil filter is a full-flow paper element type with an outer diameter of 76.0 mm {2.99 in} and height of 94.0 mm {3.70 in}.

amxzzn00000658