FUEL-FILLER LID OPENER REMOVAL/INSTALLATION

id091400804800

1. Remove the following parts:

  (1) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (2) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (3) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

amxzzw00000565

1 | Lift spring
2 | Fuel-filler lid opener

3. Install in the reverse order of removal.

4. Adjust the fuel-filler lid. (See FUEL-FILLER LID ADJUSTMENT.)