HEADLIGHT CLEANER ACTUATOR REMOVAL/INSTALLATION

id091900803000

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the front side turn light. (See SIDE TURN LIGHT REMOVAL/INSTALLATION.)

4. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

5. Pull out the headlight cleaner cover.

6. While Pulling the headlight cleaner cover, push the tab with a tape-wrapped flathead screwdriver (1), remove the headlight cleaner cover (2).

amxzzw00001186

7. Squeeze the clip tabs and slide the clip in the direction of the arrow.

amxzzw00001187

8. Disconnect headlight cleaner hose from the headlight cleaner actuator.

9. Remove the clamp.

amxzzw00001188

10. Remove the collar

11. Push the tab in the direction shown by the arrow (1), remove the tab (2), then remove the headlight cleaner actuator (3).

amxzzw00001189

12. Install in the reverse order of removal.