B1, B3 BRAKE AND F1, F2 ONE-WAY CLUTCH COMPONENT DISASSEMBLY

id051300260900

Components

bsj6za00000624

1 | Thrust washer
2 | F2 one-way clutch
3 | Thrust washer
4 | Snap ring
5 | Driven plate
6 | Drive plate
7 | Driven plate
8 | Snap ring
9 | Piston return spring
10 | B3 brake piston
11 | O-ring
12 | B3 brake cylinder
13 | F1 one-way clutch
14 | Thrust washer
15 | Bearing race
16 | Retaining plate
17 | Drive plate
18 | Driven plate
19 | Snap ring
20 | Spring return
21 | B1 brake piston
22 | O-ring
23 | B1 brake cylinder

Disassembly Procedure

1. Remove the B3 brake cylinder from the F1 one-way clutch.

bsj6za00000246

2. Remove the F1 one-way clutch and the thrust washer from the bearing race.

bsj6za00000247

3. Using a flathead screwdriver, remove the snap ring from the B3 brake cylinder.

bsj6za00000248

4. Remove the piston return spring from the B3 brake piston.

bsj6za00000249

5. While pushing the B3 brake piston, apply compressed air into the oil passage as shown in the figure and remove the B3 brake piston from the B3 brake cylinder.

bsj6za00000171

  Air pressure

  392 kPa (4.0 kgf/cm2, 57 psi)

6. Remove the O-ring from the B3 brake piston.

bsj6za00000250

7. While pushing the B1 brake piston, apply compressed airinto the oil passage as shown in the figure and remove the B1 brake piston from the B1 brake cylinder.

bsj6za00000173

  Air pressure

  392 kPa (4.0 kgf/cm2, 57 psi)

8. Remove the O-ring from the B1 brake piston.

bsj6za00000251