POWERFLOW OPERATION

id051300320600

List of operating components

Clutch / Brake | Operation
--- | ---
C1 clutch | • Engages input shaft and intermediate shaft via F4 one-way clutch.
C2 clutch | • Engages input shaft and middle planetary carrier.
C3 clutch | • Engages input shaft and front sun gear.
C4 clutch | • Engages input shaft and intermediate shaft.
B1 brake | • Locks rotation of front planetary carrier.
B2 brake | • Locks rotation of front and middle ring gear.
B3 brake | • Locks F2 one-way clutch outer race.
B4 brake | • Locks rotation of rear ring gear.
F1 one-way clutch | • Locks counterclockwise rotation of front planetary carrier on transmission case.
F2 one-way clutch | • Locks counterclockwise rotation of front sun gear during B3 brake operation.
F3 one-way clutch | • Locks counterclockwise rotation of rear ring gear. • Locks counterclockwise rotation of middle planetary carrier.
F4 one-way clutch | • Locks counterclockwise rotation of intermediate shaft during C1 clutch operation.

1GR

bsj6za00000004

bsj6za00000005

2GR

bsj6za00000006

bsj6za00000007

3GR

bsj6za00000008

bsj6za00000009

4GR

bsj6za00000010

bsj6za00000011

5GR

bsj6za00000012

bsj6za00000013

6GR

bsj6za00000014

bsj6za00000015

R position

bsj6za00000016

bsj6za00000017