FUEL-FILLER LID ADJUSTMENT

id091000800200

1. Measure the gap and height difference between the fuel-filler lid and the body.

2. Loosen the fuel-filler lid installation bolts, and adjust the fuel-filler lid.

amxzzw00002033

  Standard clearance

  a: 1.7—3.7 mm {0.07—0.14 in}
  b: -0.05—1.5 mm {0.02—0.05 in}
  c: -1.0—1.0 mm {0.04—0.03 in}
  d: -0.75—1.25 mm {-0.03—0.04 in}

3. Tighten the bolts. (See FUEL-FILLER LID REMOVAL/INSTALLATION)