CHARCOAL CANISTER INSPECTION [L8, LF]

id0116a3800500

Airflow Inspection

1. Remove the charcoal canister. (See CHARCOAL CANISTER REMOVAL/INSTALLATION [L8, LF].)

2. Perform the following procedures:

  • Assemble the hose used for inspection (bore: approx. 5.8 mm {0.23 in}) to port A.
  • Cover ports B and C with the caps.

amxzzw00000830

  Caution
  • Do not apply a pressure 20kPa {150 mmHg, 5.91 inHg} or more to the charcoal canister for 1 min. or more. Doing so will damage the charcoal canister.

3. Apply pressure (19.6 kPa {147 mmHg, 5.79 inHg}) through the hose, and verify that air does not leak from the charcoal canister.

amxzzw00000831

  • If there is airflow, replace the chacoal canister. (See CHARCOAL CANISTER REMOVAL/INSTALLATION [L8, LF].)