BUCKLE REMOVAL/INSTALLATION

id081100804400

1. Turn the ignition switch to the LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the seat. (See SEAT REMOVAL/INSTALLATION.)

5. Detach the tab as shown in the figure and remove the connector from the seat connector.

e5u811zw5007

6. Remove the bolt.

amxzzw00001799

7. Remove the buckle.

8. Install in the reverse order of removal.