MICROPHONE REMOVAL/INSTALLATION

id092000801400

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the meter hood. (See METER HOOD REMOVAL/INSTALLATION.)

4. Remove the microphone in the direction of the arrow (2) shown in the figure while pressing the microphone tabs in the direction of the arrow (1).

amxzzw00002308

5. Install in the reverse order of removal.