CENTER PANEL UNIT CONSTRUCTION

id092000101500

• A center panel unit has been adopted with the audio unit and climate control unit installed, and the audio switches and display built into the center panel.

Structural View

amxzzn00000261

Terminal Layout and Signal

Audio unit

Terminal | Signal
--- | ---
| 1A | Door speaker LH (+)
1B | B+ (Power back up)
1C | Door speaker LH (–)
1D | Door speaker RH (+)
1E | TNS (+)
1F | Door speaker RH (–)
1G | Illumination (–)
1H | Antenna control
1I | Vehicle speed signal
1J | AMP control*1
1K | —
1L | —
1M | —
1N | Audio control switch 1
1O | CAN_H*2
1P | Audio control switch 2
1Q | CAN_L*2
1R | ACC
1S | Rear speaker RH (–)*3/ Rear speaker LH (+)*1
1T | AudioPilot®2 control*1
1U | Rear speaker RH (+)*3 / Rear speaker LH (–)*1
1V | Rear speaker LH (–)*3 / Rear speaker RH (+)*1
1W | Power ground
1X | Rear speaker LH (+)*3/ Rear speaker RH (–)*1

Terminal | Signal
--- | ---
| 2A | Power ground
2B | TEL (+)*2
2C | Input signal RH (+)
2D | Input signal RH (–)
2E | Input signal LH (+)
2F | Input signal LH (–)
2G | —
2H | —
2I | —
2J | TEL (–)*2
2K | —
2L | —
2M | AUX control
2N | —
2O | —
2P | —

*1 :With Bose®
*2 :With HF/TEL unit
*3 :Without Bose®

Switch Location

amxzzn00000264

No. | Switch name
--- | ---
With RDS (radio data system) | Without RDS (radio data system)
1 | FM 1/2 switch
2 | AM switch
3 | CD switch
4 | AUX switch
5 | LOAD switch
6 | Eject switch
7 | H/PRESET switch 1
8 | M/PRESET switch 2
9 | PRESET switch 3
10 | CLOCK switch
11 | PTY switch | SCAN switch
12 | TA switch | RDM switch
13 | AUTO-M switch
14 | TEXT switch
15 | RPT/PRESET switch 4
16 | RDM/PRESET switch 5 | PRESET switch 5
17 | PRESET switch 6
18 | POWER/VOLUME switch | AUDIO CONT/TUNE switch
19 | SEEK/TRACK switch (down)
20 | DISC/FOLDER switch (up)
21 | DISC/FOLDER switch (down)
22 | SEEK/TRACK switch (up)
23 | AUDIO CONT/TUNE switch | POWER/VOLUME switch