FUEL SYSTEM OUTLINE [L8, LF]

id0114a3100100

Features

Improved serviceability | • Nylon tubes adopted for fuel hoses in the engine compartment and around the fuel tank, and quick release connectors adopted for joints
Reduction of evaporative gas | • Returnees fuel system adopted

Specification

Item | Specification
--- | ---
Injector | Type | Hi-ohmic
Type of fuel delivery | Top-feed
Type of drive | Voltage
Pressure regulator control pressure | (kPa {kgf/cm2, psi}) | Approx. 390 {3.98, 56.6}
Fuel pump type | Electric
Fuel tank capacity | (L {US gal, lmp gal}) | 50.0 {13.2, 11.0}

Fuel type

Fuel | Country | Specification
--- | --- | ---
Premium unleaded fuel (Conforming to EN 228*1), (Conforming to Fuel Quality Standards Act 2000*2) | Except China | 95 or above
China | Beijing | 95 or above
Except Beijing | 97 or above

*1 :Europe
*2 :Australia