POWER RETRACTABLE HARDTOP ADJUSTMENT

id091600809300

Top Lock

Type A

1. Remove the spring.

amxzzw00000890

2. Remove the snap ring. (See CONVERTIBLE TOP ADJUSTMENT.)

3. Remove the pin.

4. Remove the screws.

5. Remove the cover.

6. Adjust the clearance of part A by rotating the adjustment nut.

  Note
  • Turn the adjustment nut to the right to narrow the part A clearance, left to widen it.

amxzzw00000891

  Clearance

  A: 4—8 mm {0.16—0.31 in}

7. Install in the reverse order of removal.

Type B

1. Remove the spring.

amxzzw00000897

2. Remove the snap ring. (See CONVERTIBLE TOP ADJUSTMENT.)

3. Remove the pin.

4. Remove the cover.

5. Adjust the clearance of part A by rotating the adjustment nut.

  Note
  • Turn the adjustment nut to the right to narrow the part A clearance, left to widen it.

amxzzw00000891

  Clearance

  A: 4—8 mm {0.16—0.31 in}

6. Install in the reverse order of removal.

Snap ring removal note

  Caution
  • Remove the snap ring such that the dimension is maintained as indicated in the figure.

  amxzzw00000892

  • Because the snap ring is to be reused, remove it carefully so that the ring is not expanded.

1. Insert a tape-wrapped flathead screwdriver between the cover and snap ring, and remove the snap ring by prying along the perimeter so as not to damage the snap ring.

amxzzw00000893

Snap ring installation note

1. Insert the snap ring to the pin while slightly expanding the snap ring end using snap ring pliers.

amxzzw00000894

2. After securing the snap ring, verify that there is no excessive play between the snap ring and pin.

Power Retractable Hardtop

1. Loosen the installation bolts and nut for each link.

amxzzw00000895

2. Adjust the gap and height difference between the front roof panel, middle roof panel and rear window glass within the specification by moving them back and forth, left and right, and by adjusting the number of shims if necessary.

amxzzw00000896

  Clearance

  a:5.0—9.0 mm {0.20—0.35 in}
  b:-2.0—2.0 mm {-0.07—0.07 in}
  c:5.0—9.0 mm {0.20—0.35 in}
  d:-2.0—2.0 mm {-0.07—0.07 in}

3. Tighten the bolts and nuts.