DECK PANEL LIMIT SWITCH REMOVAL/INSTALLATION

id091600821100

  Caution
  • If the deck panel does not operate electrically, see “DECK PANEL MANUAL OPEN/CLOSE PROCEDURE” to open/close the deck panel. (See DECK PANEL MANUAL OPEN/CLOSE PROCEDURE.)

1. Fully open the deck panel.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Set the side shelf out of the way. (See SIDE SHELF REMOVAL/INSTALLATION.)

5. Remove the deck panel. (See DECK PANEL REMOVAL/INSTALLATION.)

6. Remove the deck panel motor. (RH) (See DECK PANEL MOTOR REMOVAL/INSTALLATION.)

7. Remove the screws A and B.

amxuuw00000623

8. Remove the deck panel limit switch prate.

9. Remove the screws C.

10. Remove the deck panel limit switch.

11. Install in the reverse order of removal.