SPARK PLUG REMOVAL/INSTALLATION [L8, LF]

id0118a3800400

  Caution
  • If a spark plug that is not as specified is installed, engine performance will be deteriorated. Install only the specified spark plug when replacing.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF].)

4. Remove the front suspension tower bar (joint). (See FRONT SUSPENSION TOWER BAR REMOVAL/INSTALLATION.)

5. Remove the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [L8, LF].)

6. Remove the spark plugs using a plug-wrench.

7. Install in the reverse order of removal.

  Tightening torque

  10—14 N·m {1.1—1.4 kgf·m, 8—10 ft·lbf}