DOUBLE WISHBONE FRONT SUSPENSION CONSTRUCTION

id021300629700

Improved roadholding
• The heightened damper lever ratio has improved the efficiency of shock absorber operation.

  ― Damper lever ratio:
  shock absorber stroke (B)/wheel vertical stroke (A)

  amxzzn00000292

  ― The heightened damper lever ratio has made it possible to provide a damping force even during minute strokes. As a result, excellent roadholding is exhibited in a variety of driving conditions.

Optimized roll axis position
• The height of the front roll center is set lower than the rear.
• Change of roll center height in response to a change in wheel stroke has been suppressed in order to improve roll linearity and convergence.

amxzzn00000293