DTC TABLE [POWER RETRACTABLE HARDTOP]

id0902j2960500

DTC | description | Page
--- | --- | ---
M-MDS display
B1342 | Power retractable hardtop control module internal malfunction | (See DTC B1342 [POWER RETRACTABLE HARDTOP].)
B1317 | Battery power supply voltage increases (17.5 V or more) | (See DTC B1317/B1318 [POWER RETRACTABLE HARDTOP].)
B1318 | Battery power supply voltage decreases (less than 7.5 V)
B296D | Hall sensor low power supply voltage | (See DTC B296D [POWER RETRACTABLE HARDTOP].)
U0030 | Power window communication error (during power retractable hardtop operation) | (See DTC U0030/U0031 [POWER RETRACTABLE HARDTOP].)
U0031 | Power window communication error (during power retractable hardtop not operation)
B296A | Roof motor pulse signal error (RH) | (See DTC B296A/B294B/B293C/B293B [POWER RETRACTABLE HARDTOP].)
B294B | Roof motor pulse signal error (LH)
B293C | Deck panel motor pulse signal error (RH)
B293B | Deck panel motor pulse signal error (RL)
B293E | Roof motor circuit malfunction (RH) | (See DTC B293E/B293D/B294C/B293F [POWER RETRACTABLE HARDTOP].)
B293D | Roof motor circuit malfunction (LH)
B294C | Deck panel motor circuit malfunction (RH)
B293F | Deck panel motor circuit malfunction (LH)
B294D | Roof motor opening angle does not match (Pulse count number do not match) | (See DTC B294D/B294E [POWER RETRACTABLE HARDTOP].)
B294E | Deck panel motor opening angle does not match (Pulse count number do not match)
B294F | Power retractable hardtop/deck panel limit switch malfunction | (See DTC B294F [POWER RETRACTABLE HARDTOP].)
B296B | Top lock switch malfunction | (See DTC B296B [POWER RETRACTABLE HARDTOP].)
B296C | Power retractable hardtop switch malfunction | (See DTC B296C [POWER RETRACTABLE HARDTOP].)
U0073 | CAN system communication error | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100 | Communication error to PCM
U0101 | Communication error to TCM
U2197 | Vehicle speed signal communication error