SCHEDULED MAINTENANCE

id000000801200

Scheduled Maintenance Table for Europe (L.H.D., U.K.)

Maintenance Interval | Number of months or kilometers (miles), whichever comes first
--- | ---
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108
×1000 km | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180
×1000 miles | 12.5 | 25 | 37.5 | 50 | 62.5 | 75 | 87.5 | 100 | 112.5
Engine valve clearance | Audibly inspect every 120,000 km (75,000 miles), if noisy, adjust
Engine oil *1 | R | R | R | R | R | R | R | R | R
Engine oil filter *1 | R | R | R | R | R | R | R | R | R
Drive belts *2 |  |  | I |  |  | I |  |  | I
Cooling system |  | I |  | I |  | I |  | I |
Engine coolant | FL22 type *3 | Replace every 200,000 km (125,000 miles) or 11 years
Others | Replace at first 100,000 km (62,500 miles) or 4 years; after that, every 2 years
Air cleaner element *4 | C | C | R | C | C | R | C | C | R
Fuel lines and hoses |  | I |  | I |  | I |  | I |
Spark plugs *5 | Replace every 100,000 km (62,500 miles)
Evaporative system (if installed) |  |  | I |  |  | I |  |  | I
Battery electrolyte level and specific gravity | I | I | I | I | I | I | I | I | I
Brake lines, hoses and connections | I | I | I | I | I | I | I | I | I
Brake fluid *6 |  | R |  | R |  | R |  | R |
Parking brake | I | I | I | I | I | I | I | I | I
Disc brakes | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |
Manual transmission oil |  |  |  |  | R |  |  |  |
Rear differential oil |  |  |  | R |  |  |  | R |
Front and rear suspension, ball joints and wheel bearing axial play |  | I |  | I |  | I |  | I |
Drive shaft dust boots |  | I |  | I |  | I |  | I |
Exhaust system and heat shields | Inspect every 80,000 km (50,000 miles) or 5 years
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |
Body condition (for rust, corrosion and perforation) | Inspect annually
Tires (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I
Flat tire repair kit (if installed) *7 | Inspect annually

Chart symbols
I: Inspect: Inspect and clean, repair, adjust, fill up, or replace if necessary.
R: Replace
C: Clean
T: Tighten
Remarks
Emission control and related systems
•
• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation.
All inspections and adjustments must be made by an expert repairer, we recommend an Authorized Mazda Repairer.
• After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.

  *1: If the vehicle is operated primarily under any of the following conditions, replace the engine oil and oil filter at every 10,000 km (6,250 miles) or shorter.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *2: Also inspect and adjust the power steering and air conditioner drive belts, if installed.
  If the vehicle is operated primarily under any of the following conditions, inspect the drive belts at every 20,000 km (12,500 miles) or 12 months.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *3: Use FL22 type coolant in vehicles with the inscription “FL22” on the radiator cap itself or the surrounding area. Use FL22 when replacing the coolant.
  *4: If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
  *5: In the countries below, inspect the spark plugs at every 20,000 km (12,500 miles) or 12 months before replacing them at the said interval.
  Croatia, Macedonia, Bosnia and Herzegovina, Serbia, Montenegro, Bulgaria, Romania
  *6: If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, replace the brake fluid annually.
  *7: Check the tire repair fluid expiration date every year when performing the periodic maintenance. Replace the tire repair fluid bottle with new one before the expiration date.

Scheduled Maintenance Table for Israel

Maintenance Interval | Number of months or kilometers (miles), whichever comes first
--- | ---
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
×1000 km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120 | 135 | 150 | 165 | 180
×1000 miles | 9.4 | 18.8 | 28.1 | 37.5 | 46.9 | 56.3 | 65.6 | 75.0 | 84.4 | 93.8 | 103.1 | 112.5
Engine valve clearance | Audibly inspect every 120,000 km (75,000 miles), if noisy, adjust
Engine oil *1 | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter *1 | R | R | R | R | R | R | R | R | R | R | R | R
Drive belts *2 | I | I | I | I | I | I | I | I | I | I | I | I
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | FL22 type *3 | Replace every 195,000 km (121,900 miles) or 10 years
Others | Replace at first 90,000 km (56,300 miles) or 4 years; after that, every 2 years
Air cleaner element *4 | C | C | C | R | C | C | C | R | C | C | C | R
Fuel filter | Replace every 105,000 km (65,600 miles)
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I
Spark plugs | Replace every 90,000 km (56,300 miles) or 3 years
Evaporative system (if installed) |  |  |  | I |  |  |  | I |  |  |  | I
Battery electrolyte level and specific gravity | I | I | I | I | I | I | I | I | I | I | I | I
Brake lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I
Brake fluid *5 | I | R | I | R | I | R | I | R | I | R | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses | I | I | I | I | I | I | I | I | I | I | I | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I
Manual transmission oil |  |  |  |  |  | R |  |  |  |  |  | R
Rear differential oil |  |  |  |  | R |  |  |  |  | R |  |
Front and rear suspension, ball joints and wheel bearing axial play | I | I | I | I | I | I | I | I | I | I | I | I
Drive shaft dust boots |  |  | I |  |  | I |  |  | I |  |  | I
Exhaust system and heat shields | Inspect every 75,000 km (46,900 miles)
Bolts and nuts on chassis and body | T | T | T | T | T | T | T | T | T | T | T | T
Body condition (for rust, corrosion and perforation) | Inspect annually
Tires (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I | I | I | I
Flat tire repair kit (if installed) *6 | Inspect annually

Chart symbols
I: Inspect: Inspect and clean, repair, adjust, fill up, or replace if necessary.
R: Replace
C: Clean
T: Tighten
Remarks
• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation.
All inspections and adjustments must be made by an expert repairer, we recommend an Authorized Mazda Repairer.
• After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.
Emission control and related systems
*1: If the vehicle is operated primarily under any of the following conditions, replace the engine oil and oil filter at every 10,000 km (6,250 miles) or shorter.

  a. Driving in dusty conditions
  b. Extended periods of idling or low speed operation
  c. Driving for long period in cold temperatures or driving regularly at short distance only
  d. Driving in extremely hot conditions
  e. Driving in mountainous conditions continually

*2: Also inspect and adjust the power steering and air conditioner drive belts, if installed.
If the vehicle is operated primarily under any of the following conditions, inspect the drive belts at every 10,000 km (6,250 miles) or shorter.

  a. Driving in dusty conditions
  b. Extended periods of idling or low speed operation
  c. Driving for long period in cold temperatures or driving regularly at short distance only
  d. Driving in extremely hot conditions
  e. Driving in mountainous conditions continually

*3: Use FL22 type coolant in vehicles with the inscription “FL22” on the radiator cap itself or the surrounding area. Use FL22 when replacing the coolant.
*4: If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
*5: If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, replace the brake fluid annually.
*6: Check the tire repair fluid expiration date every year when performing the periodic maintenance. Replace the tire repair fluid bottle with new one before the expiration date.

Scheduled Maintenance Table for Russia

Maintenance Interval | Number of months or kilometers (miles), whichever comes first
--- | ---
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
×1000 km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120 | 135 | 150 | 165 | 180
×1000 miles | 9 | 18 | 27 | 36 | 45 | 54 | 63 | 72 | 81 | 90 | 99 | 108
Engine valve clearance | Audibly inspect every 45,000 km (27,000 miles) or 3 years, if noisy, adjust
Engine oil *1 | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter *1 | R | R | R | R | R | R | R | R | R | R | R | R
Drive belts *2 | I | I | I | I | I | I | I | I | I | I | I | I
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | FL22 type *3 | Replace every 195,000 km (117,000 miles) or 11 years
Others | Replace at first 90,000 km (54,000 miles) or 4 years; after that, every 2 years
Air cleaner element *4 | C | C | R | C | C | R | C | C | R | C | C | R
Fuel filter | Replace every 60,000 km (36,000 miles)
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I
Spark plugs | I | I | I | I | R | I | I | I | I | R | I | I
Evaporative system (if installed) |  |  |  | I |  |  |  | I |  |  |  | I
Battery electrolyte level and specific gravity | I | I | I | I | I | I | I | I | I | I | I | I
Brake lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I
Brake fluid *5 |  | R |  | R |  | R |  | R |  | R |  | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages | I | I | I | I | I | I | I | I | I | I | I | I
Manual transmission oil | I | I | I | I | R | I | I | I | I | R | I | I
Rear differential oil |  |  |  |  | R |  |  |  |  | R |  |
Front and rear suspension, ball joints and wheel bearing axial play | I | I | I | I | I | I | I | I | I | I | I | I
Drive shaft dust boots | I | I | I | I | I | I | I | I | I | I | I | I
Exhaust system and heat shields | I | I | I | I | I | I | I | I | I | I | I | I
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |  | T |  | T
Hinges and catches |  | L |  | L |  | L |  | L |  | L |  | L
All electrical system | I | I | I | I | I | I | I | I | I | I | I | I
Body condition (for rust, corrosion and perforation) | Inspect annually
Tires (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I | I | I | I
Flat tire repair kit (if installed) *6 | Inspect annually

Chart symbols
I: Inspect: Inspect and clean, repair, adjust, fill up, or replace if necessary
R: Replace
C: Clean
T: Tighten
L: Lubricate
Remarks
Emission control and related systems
• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation.
All inspections and adjustments must be made by an expert repairer, we recommend an Authorized Mazda Repairer.
• After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.

  *1: If the vehicle is operated primarily under any of the following conditions, replace the engine oil and oil filter at every 7,500 km (4,500 miles) or 6 months.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *2: Also inspect and adjust the power steering and air conditioner drive belts, if installed.
  If the vehicle is operated primarily under any of the following conditions, inspect the drive belts at every 7,500 km (4,500 miles) or 6 months.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *3: Use FL22 type coolant in vehicles with the inscription “FL22” on the radiator cap itself or the surrounding area. Use FL22 when replacing the coolant.
  *4: If the vehicle is operated in very dusty or sandy areas, clean the air cleaner element at every 7,500 km (4,500 miles) or 6 months.
  *5: If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, replace the brake fluid annually.
  *6: Check the tire repair fluid expiration date every year when performing the periodic maintenance. Replace the tire repair fluid bottle with new one before the expiration date.

Scheduled Maintenance Table for General (L.H.D., R.H.D.)

Maintenance Interval | Number of months or kilometers (miles), whichever comes first
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
×1000 miles | 6.25 | 12.5 | 18.75 | 25 | 31.25 | 37.5 | 43.75 | 50 | 56.25 | 62.5 | 68.75 | 75 | 81.25 | 87.5 | 93.75 | 100
Engine valve clearance | Audibly inspect every 120,000 km (75,000 miles), if noisy, adjust
Engine oil *1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter *1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Drive belts *2 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | FL22 type *3 |  |  |  |  |  |  |  |  |  | R |  |  |  |  |  |
Others | Replace every 2 years
Air cleaner element *4 |  | C |  | C |  | R |  | C |  | C |  | R |  | C |  | C
Fuel filter | Replace every 60,000 km (37,500 miles)
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Spark plugs | Replace every 100,000 km (62,500 miles)
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Battery electrolyte level and specific gravity *5 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake lines, hoses and connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid *6 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Manual transmission oil |  |  |  |  |  |  |  |  |  | R |  |  |  |  |  |
Rear differential oil |  |  |  |  |  |  |  | R |  |  |  |  |  |  |  | R
Front and rear suspension, ball joints and wheel bearing axial play |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Drive shaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Exhaust system and heat shields | Inspect every 80,000 km (50,000 miles)
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
Body condition (for rust, corrosion and perforation) | Inspect annually
Tire rotation | Rotate every 10,000 km (6,250 miles)
Tires (including spare tire) (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Flat tire repair kit (if installed) *7 | Inspect annually

Chart symbols
I: Inspect: Inspect and clean, repair, adjust, fill up, or replace if necessary.
R: Replace
C: Clean
T: Tighten
Remarks
Emission control and related systems
• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation.
All inspections and adjustments must be made by an expert repairer, we recommend an Authorized Mazda Repairer.
• After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.

  *1: If the vehicle is operated primarily under any of the following conditions, replace the engine oil and oil filter more often than the recommended intervals.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *2: Also inspect and adjust the power steering and air conditioner drive belts, if installed.
  If the vehicle is operated primarily under any of the following conditions, inspect the drive belts more often than the recommended intervals.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *3: Use FL22 type coolant in vehicles with the inscription “FL22” on the radiator cap itself or the surrounding area. Use FL22 when replacing the coolant.
  *4: If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
  *5: If the vehicle is operated in extremely heat and extremely cold areas, inspect the battery electrolyte level and specific gravity at every 10,000 km (6,250 miles) or 6 months.
  *6: If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, replace the brake fluid annually.
  *7: Check the tire repair fluid expiration date every year when performing the periodic maintenance. Replace the tire repair fluid bottle with new one before the expiration date.

Scheduled Maintenance Table for Australia

Maintenance Interval | Number of months or kilometers, whichever comes first
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
Engine valve clearance | Audibly inspect every 120,000 km, if noisy, adjust
Engine oil *1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter *1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Drive belts *2 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | FL22 type *3 | Replace at first 200,000 km or 10 years; after that, every 100,000 km or 5 years
Others | Replace at first 80,000 km or 4 years; after that, every 2 years
Air cleaner element *4 |  | C |  | C |  | R |  | C |  | C |  | R |  | C |  | C
Fuel filter | Replace every 150,000 km
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Spark plugs | Replace every 100,000 km
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Battery electrolyte level and specific gravity |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake lines, hoses and connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid *5 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Manual transmission oil |  |  |  |  |  |  |  |  |  | R |  |  |  |  |  |
Rear differential oil |  |  |  |  |  |  |  | R |  |  |  |  |  |  |  | R
Front and rear suspension, ball joints and wheel bearing axial play |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Drive shaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Exhaust system and heat shields | Inspect every 80,000 km
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
All electrical system *6 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Tire rotation *7 | Rotate every 10,000 km or 6 months
Tires (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Flat tire repair kit (if installed) *8 | Inspect annually
Road test | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
M-MDS check of Vehicle Management and Safety Systems |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I

Chart symbols
I: Inspect: Inspect and clean, repair, adjust, fill up, or replace if necessary.
R: Replace
C: Clean
T: Tighten
Remarks
Emission control and related systems
• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation.
All inspections and adjustments must be made by an expert repairer, we recommend an Authorized Mazda Repairer.
• After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.

  *1: If the vehicle is operated primarily under any of the following conditions, replace the engine oil and oil filter more often than the recommended intervals.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *2: Also inspect and adjust the power steering and air conditioner drive belts, if installed.
  If the vehicle is operated primarily under any of the following conditions, inspect the drive belts more often than the recommended intervals.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *3: Use FL22 type coolant in vehicles with the inscription “FL22” on the radiator cap itself or the surrounding area. Use FL22 when replacing the coolant.
  *4: If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
  *5: If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, replace the brake fluid annually.
  *6: This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.
  *7: If the vehicle is operated primarily under any of the following conditions, rotate the tires more often than the recommended intervals.
    a. Driving on bumpy roads, gravel roads, snowy roads or dirt roads
    b. Driving uphill and downhill frequently
    c. Repeated short-distance driving
    d. On roads having many roundabouts
  *8: Check the tire repair fluid expiration date every year when performing the periodic maintenance. Replace the tire repair fluid bottle with new one before the expiration date.

Advice
• Please ask Mazda dealer to check Mazda computer network to ensure there are no outstanding campaign or recall actions on the vehicle.

Scheduled Maintenance Table For China

Maintenance Interval | Number of months or kilometers, whichever comes first
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
Engine valve clearance | Audibly inspect every 120,000 km, if noisy, adjust
Drive belts *1 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Engine oil *2 | Replace every 5,000 km or 6 months
Engine oil filter *2 | Replace every 10,000 km or 12 months
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | FL22 type *3 | Replace at first 200,000 km or 10 years; after that, every 100,000 km or 5 years
Others | Replace at first 200,000 km or 10 years; after that, every 2 years
Air cleaner element *4 |  | C |  | R |  | C |  | R |  | C |  | R |  | C |  | R
Spark plugs *5 | Replace every 100,000 km
Fuel filter |  |  |  | R |  |  |  | R |  |  |  | R |  |  |  | R
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Battery electrolyte level and specific gravity |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake lines, hoses and connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid *6 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Rear differential oil |  |  |  |  |  |  |  | R |  |  |  |  |  |  |  | R
Front and rear suspension, ball joints and wheel bearing axial play |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Drive shaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Exhaust system and heat shields |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
All electrical system*7 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Body condition (for rust, corrosion and perforation) | Inspect annually
Tires (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Tire rotation | Rotate every 10,000 km
Flat tire repair kit *8 | Inspect annually

Chart symbols
I: Inspect: Inspect and clean, repair, adjust, fill up, or replace if necessary.
R: Replace
T: Tighten
C: Clean
Remarks
• To ensure efficient operation of the engine and all systems related to emission control, the ignition and fuel systems must be serviced regularly. It is strongly recommended that all servicing related to these systems be done by an authorized Mazda Dealer.
• After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.

  *1: Also inspect and adjust the power steering and air conditioner drive belts, if installed.If the vehicle is operated primarily under any of the following conditions, inspect the drive belts more often than the recommended intervals.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *2: If the vehicle is operated primarily under any of the following conditions, replace the engine oil at every 2,500 km or 3 months and replace the oil filter at every 5,000 km or 6 months.
    a. Driving in dusty conditions
    b. Extended periods of idling or low speed operation
    c. Driving for long period in cold temperatures or driving regularly at short distance only
    d. Driving in extremely hot conditions
    e. Driving in mountainous conditions continually
  *3: Use FL22 type coolant in vehicles with the inscription “FL22” on the radiator cap itself or the surrounding area. Use FL22 when replacing the coolant.
  *4: If the vehicle is operated in very dusty or sandy areas, clean the air cleaner element at every 10,000 km or 6 months.
  *5: If gasoline with high iron or manganese is used, inspect the spark plugs at every 10,000 km or 6 months, and replace them if necessary.
  *6: If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, replace the brake fluid annually.
  *7: This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.
  *8: Check the tire repair fluid expiration date every year when performing the periodic maintenance. Replace the tire repair fluid bottle with new one before the expiration date.

Scheduled Maintenance Service (Specific Work Required)

• The specific work required for each maintenance item is listed in the following table. (Please refer to the section applicable to the model serviced.)

Maintenance Item | Specific Work Required
--- | ---
ENGINE
Engine valve clearance | Inspect engine valve clearance.
Engine timing belt | Replace engine timing belt.
Engine timing belt auto tensioner | Replace engine timing belt auto tensioner.
Drive belts | Inspect for wear, cracks, fraying and tension.
Engine oil | Replace engine oil and inspect for leakage.
Engine oil filter | Replace engine oil filter and inspect for leakage.
COOLING SYSTEM
Cooling system (Including coolant level adjustment) | Check engine coolant level and quality, and inspect for leakage.
Radiator cap | Inspect radiator cap.
Engine coolant | Replace engine coolant.
FUEL SYSTEM
Idle speed | Check engine idle rpm.
Idle mixture | Inspect the CO and HC concentrations (see W/M).
Choke system | Check system operation.
Air cleaner element | Inspect dirt, oil and damage. Clean air cleaner element (by blowing air). Replace air cleaner element.
Fuel filter | Replace fuel filter.
Fuel injection pump inlet filter | Clean fuel injection pump inlet filter.
Fuel lines and hoses Fuel lines, hoses and connections | Inspect for cracks, leakage and loose connection.
Fuel injection system | Update to injection amount correction with WDS (see W/M). Update to injection amount correction with M-MDS (see W/M).
Fuel system (Drain water) | Drain water in fuel system.
Diesel particulate filter | Replace diesel particulate filter.
Fuel additive for diesel particulate filter | Fill up fuel additive.
IGNITION SYSTEM
Initial ignition timing | Check initial ignition timing.
Spark plugs | Inspect for wear, damage, carbon, plug gap and high-tension lead condition. Replace spark plugs.
Ignition cables condition/security | Inspect for damage, condition and connection.
EMISSION CONTROL SYSTEM
Evaporative system Evaporative emission control system | Check system operation (see W/M), vapor lines, vacuum fitting hoses and connection.
Crankcase emission control system | Check system operation (see W/M), PCV valve, blow-by lines, vacuum fitting hoses and connection.
E.G.R system | Check system operation (see W/M), vacuum fitting hoses and connection. MZR-CD (RF turbo) engine: Update to MAF correction for E.G.R control with WDS (see W/M). MZR-CD (RF turbo) engine: Update to MAF correction for E.G.R control with M-MDS (see W/M).
Air intake system | Update to MAF correction (see W/M).
Throttle positioner system | Check the diaphragm and system operation, vacuum fitting hoses and connection.
Dash pot | Check system operation.
ELECTRICAL SYSTEM
Battery electrolyte level and specific gravity | Check battery electrolyte level and specific gravity.
Battery condition | Check battery for corroded or loose connections and cracks.
Battery | Check battery for leakage and corrosion.
All electrical system Lighting system and windshield wipers and washer | Check function of lighting system, windshield wiper (including wiper blade condition), washer and power windows.
Head light alignment | Check head light alignment.
CHASSIS AND BODY
Brake and clutch pedals Brake pedals | Check pedal height and free play.
Brake fluid | Check brake fluid level and for leakage. Replace brake fluid.
Clutch fluid | Check Clutch fluid level and for leakage.
Brake lines, hoses and connections | Inspect for cracks, damage, chafing, corrosion, scars, swelling and fluid leakage.
Parking brake | Check parking lever stroke.
Power brake unit and hoses Power brake unit (Brake booster) and hoses | Check vacuum lines, connections, and check valve for improper attachment, air tightness, cracks chafing and deterioration.
Disc brakes | Inspect caliper for correct operation and fluid leakage, brake pads for wear. Check disc plate condition and thickness. Test for judder and noise.
Drum brakes | Inspect brake drum for wear and scratches: brake lining for wear, peeling and cracks; wheel cylinder for fluid leakage. Test for judder and noise.
Manual steering gear oil | Check manual gear oil level.
Power steering fluid, lines, hoses and connections Power steering fluid and lines | Check power steering fluid level and lines for improper attachment, leakage, cracks, damage, loose connections, chafing and deterioration.
Steering operation and gear housing Steering linkages tie rod ends and arms Steering operation and linkages | Check that the steering wheel has the specified play. Be sure to check for changes, such as excessive play, hard steering or strange noises. Check gear housing and boots for looseness, damage and grease/gear oil leakage. Check ball joint, dust cover and other components for looseness, wear, damage and grease leakage.
Front and rear suspension and ball joints Front suspension ball joints Front and rear suspension, ball joints and wheel bearing axial play | Inspect for grease leakage, crack, damage and looseness. Inspect for grease leakage, crack, damage, looseness and wheel bearing play/noise.
Wheel bearing axial play | Inspect for wheel bearing play/noise.
Manual transmission/transaxle oil | Check manual transmission/transaxle oil level and for leakage. Replace manual transmission/transaxle oil.
Front and rear differential oil Front differential oil Front axle oil Rear differential oil Rear axle oil | Check front and rear differential oil level and inspect for leakage. Replace front and rear differential oil.
Transfer oil | Check transfer oil level inspect for leakage. Replace transfer oil
Front and rear wheel bearing grease Front wheel bearing grease | Remove wheel bearing and replace wheel bearing grease.
Wheel bearing axial play Wheel bearing axial play (rear) and lateral play (front) | Inspect wheel bearing play and noise.
Propeller shaft joints Front propeller shaft joints Rear propeller shaft joints | Lubricate propeller shaft joints.
Drive shaft dust boots | Inspect for grease leakage, crack, damage and looseness.
Wheel nuts | Tighten wheel nuts.
Bolts and nuts on chassis and body Bolts and nuts on seats | Tighten bolts and nuts fastening suspension components, members and seat frames.
Body condition (for rust, corrosion and perforation) | Inspect body surface for paint damage, rust, corrosion and perforation.
Exhaust system and heat shields Exhaust pipe connections | Inspect for damage, corrosion, looseness of connections and gas leakage.
Tire rotation | Rotate tires.
Tires (Including spare tire)(with inflation pressure adjustment) | Check air pressure and inspect tires for tread wear, damage, cracks; and wheels for damage and corrosion.
Flat tire repair kit | Check tire repair fluid expiration date.
Hinges and catches | Lubricate hinges and catches of doors, trunk lid and hood.
Underside of vehicle | Inspect underside of vehicle (floor pans, frames, fuel lines, around exhaust system etc.) for damage and corrosion.
Road test | Check brake operation/clutch operation/steering control/operation of meters and gauges/squeaks, rattles, or unusual noises/engine general performance/emergency locking retractors.
Diagnostic trouble code by WDS Diagnostic trouble code by M-MDS | Check diagnostic trouble code with WDS (see W/M). Check diagnostic trouble code with M-MDS (see W/M).
M-MDS check of Vehicle Management and Safety Systems | Check the items below with M-MDS (see W/M). (1) Retrieve All CMDTCs (2) PCM function test (except Tribute and diesel engine models) (3) PCM Input/Output Data Monitor (except Tribute and diesel engine models) (4) Adviser Comment (except Tribute and diesel engine models)
AIR CONDITIONER SYSTEM
Cabin air filter | Replace cabin air filter.