INSTRUMENT CLUSTER CONFIGURATION

id092200496200

1. Connect the M-MDS to the DLC-2.

amxzzw00001703

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select “Module Programming”.
  • When using the PDS (Pocket PC)
    1. Select “Programming”.
    2. Select “Module Programming”.

3. Select “Programmable Module Installation”.

4. Select “IC” and perform procedures according to directions on the M-MDS screen.

5. Retrieve DTCs using the M-MDS and verify that there is no DTC present.

  • If any DTC is present, perform applicable DTC inspection. (See DTC INSPECTION [INSTRUMENT CLUSTER].)