WASHER HOSE REMOVAL/INSTALLATION

id091900804900

1. Remove the wiper arm and blade. (See WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Disconnect joint pipe A, then remove washer hose A from clip A.

e5u919zw5013

3. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

4. Remove clips.

5. Disconnect joint pipe B, then remove washer hose A.

6. Disconnect washer hose B from the washer nozzle, then remove washer hose B.

7. Disconnect joint pipe C, then remove washer hose C.

8. Remove washer hose D from clips C.

9. Disconnect washer hose D from the washer nozzle, then remove washer hose D.

10. Install in the reverse order of removal.