DTC P0717 [SJ6A-EL]

id050208801500

DTC P0717 | Turbine sensor circuit malfunction (open circuit/short circuit)
--- | ---
DETECTION CONDITION | • When all conditions below are satisfied. ― D range of TR switch input ― Vehicle speed signal 12 pulse input ― Turbine sensor signal not input Diagnostic support note: • The MIL illuminates if the TCM detects the above malfunction condition during the first drive cycle. • The AT warning light illuminates if the TCM detects the above malfunction condition during the first drive cycle. • PENDING CODE is not available. • FREEZE FRAME DATA is available. • The DTC is stored in the TCM memory.
POSSIBLE CAUSE | • TCM connector or terminal malfunction • Short to GND in wiring harness between turbine sensor terminal B and TCM terminal 2A • Short to GND in wiring harness between turbine sensor terminal A and TCM terminal 2B • Short to power supply in wiring harness between turbine sensor terminal B and TCM terminal 2A • Short to power supply in wiring harness between turbine sensor terminal A and TCM terminal 2B • Turbine sensor connector or terminal malfunction • Turbine sensor malfunction • Open circuit between turbine sensor terminal B and TCM terminal 2A • Open circuit between turbine sensor terminal A and TCM terminal 2B • TCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has the FREEZE FRAME DATA been recorded on the repair order? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT TCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch to the LOCK position. • Disconnect the TCM connector. • Inspect for poor connection at TCM terminals R18 and R7 (such as damaged/pulled-out pins, corrosion). • Are terminals normal? | Yes | Go to the next step.
No | Repair or replace the connector and/or terminal, then go to Step 13.
4 | INSPECT CONTINUITY OF TURBINE SENSOR CIRCUIT • Inspect for continuity between the TCM terminals 2A and 2B (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Go to Step 7.
5 | INSPECT TURBINE SENSOR SIGNAL CIRCUIT FOR SHORT TO GND • Inspect for continuity between the TCM terminals (wiring harness-side) and body GND. ― Terminal 2A and body GND ― Terminal 2B and body GND • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for short to GND, then go to Step 10.
6 | INSPECT TURBINE SENSOR CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the ignition switch to the ON position (engine off). • Measure the voltage at TCM (wiring harness-side) terminals 2A and 2B. • Is there 0 V at the TCM wiring harness-side connector terminals? | Yes | Go to the next step.
No | Repair or replace the wiring harness for short to power supply, then go to Step 10.
7 | INSPECT TERMINAL TURBINE SENSOR FOR POOR CONNECTION • Turn the ignition switch to the LOCK position. • Disconnect the turbine sensor connector. • Inspect for poor connection at turbine sensor terminals A and B (such as damaged/pulled-out pins, corrosion). • Are terminals normal? | Yes | Go to the next step.
No | Repair or replace the connector and/or terminal, then go to Step 10.
8 | INSPECT TURBINE SENSOR • Inspect the turbine sensor. (See TURBINE SENSOR INSPECTION [SJ6A-EL].) • Is the turbine sensor normal? | Yes | Go to the next step.
No | Replace the turbine sensor, then go to Step 10. (See TURBINE SENSOR REMOVAL/INSTALLATION [SJ6A-EL].)
9 | INSPECT TURBINE SENSOR CIRCUIT FOR OPEN CIRCUIT • Inspect for continuity between turbine sensor terminals (wiring harness-side) and TCM terminals (wiring harness-side). ― Terminal B and terminal 2A ― Terminal A and terminal 2B • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for open circuit, then go to the next step.
10 | VERIFY TROUBLESHOOTING OF DTC P0717 COMPLETED • Make sure to reconnect all the disconnected connectors. • Clear the DTC using the M-MDS. • Perform the following procedure to ensure that the DTC has been resolved: 1. Start the engine. 2. Warm-up the engine and transmission. 3. Drive the vehicle in D range and make sure that the gears shift smoothly from 1GR to 6GR. • Is the same DTC present? | Yes | Replace the TCM, then go to the next step. (See TCM REMOVAL/INSTALLATION [SJ6A-EL].)
No | Go to the next step.
11 | VERIFY NO DTC HAS BEEN PRESENTED • Perform the “Reading DTCs Procedure”. (See AUTOMATIC TRANSMISSION ON-BOARD DIAGNOSTIC FUNCTION [SJ6A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [SJ6A-EL].)
No | DTC troubleshooting completed.