ROOF MOTOR REMOVAL/INSTALLATION

id091600809700

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (8) Seat belt upper anchor installation bolt (See SEAT BELT REMOVAL/INSTALLATION.)

  (9) Power retractable hardtop link bracket (See POWER RETRACTABLE HARDTOP LINK BRACKET REMOVAL/INSTALLATION.)

4. Disconnect the roof motor connector.

5. Remove the bolts A and washers.

amxzzw00002097

6. Remove the roof motor bracket.

7. Remove the bolts B and C.

8. Remove the roof motor.

9. Install in the reverse order of removal.