REAR DECK WEATHERSTRIP INSTALLATION

id091600811200

1. Align the deck flange with the weatherstrip marking, and insert. (1)

amxzzw00000915

2. Peel off the tape backing of the butylene tape, align it to the molded part at the tip of the rear deck weatherstrip and press, then attach the fasteners. (2)

3. Install the rear deck weatherstrip. (3)

4. Install the cab-side weatherstrip. (See CONVERTIBLE TOP DISASSEMBLY/ASSEMBLY.)

5. Install the quarter trim. (See QUARTER TRIM REMOVAL/INSTALLATION.)