MIDDLE ROOF PANEL DISASSEMBLY/ASSEMBLY

id091600811000

1. Remove the middle roof panel weatherstrip. (See MIDDLE ROOF PANEL WEATHERSTRIP REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

3. Assemble in the reverse order of disassembly.

amxzzw00000936

1 | Retainer (See Retainer Disassembly Note.) (See Retainer Assembly Note.)
2 | Middle roof panel

Retainer Disassembly Note

1. Mark around the retainer installation screws with paint before removing them.

amxzzw00000937

Retainer Assembly Note

1. Install the retainers to the link, aligning the retainer marks with the retainer installation screws.

amxzzw00000937