KEYLESS RECEIVER REMOVAL/INSTALLATION

id091400438300

L.H.D.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the glove compartment lid. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Disconnect the keyless receiver module connector.

4. Remove the nut, then remove the keyless receiver (front).

amxzzw00000577

5. Install in the reverse order of removal.

R.H.D.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the nut, then pull the keyless receiver.

amxzzw00000578

4. Disconnect the keyless receiver module connector.

5. Install in the reverse order of removal.