TAPPET INSPECTION

id011000505800

1. Measure the tappet hole inner diameter in X and Y directions at the two points (A and B) shown in the figure.

belbze00000141

  Inner diameter

  31.000—31.030 mm {1.2205—1.2216 in}

2. Measure the tappet body outer diameter in X and Y directions at the two points (A and B) shown in the figure.

belbze00000142

  Outer diameter

  30.970—30.980 mm {1.2193—1.2196 in}

3. Subtract the tappet body outer diameter from the tappet hole inner diameter.

  • If it exceeds the specification, replace the tappet or cylinder head.

  Standard clearance
  0.02—0.06 mm {0.0008—0.0023 in}

  Maximum clearance
  0.15 mm {0.006 in}