WHEEL HUB, STEERING KNUCKLE REMOVAL/INSTALLATION

id031100800400

  Caution
  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before performing the following procedures, disconnect the ABS wheel-speed sensor harness connector (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, inspect front wheel alignment. (See FRONT WHEEL ALIGNMENT.)

amxzzw00001234

1 | ABS wheel-speed sensor
2 | Brake calliper component (See Brake Caliper Component Removal Note.)
3 | Disc plate
4 | Tie-rod end (See STEERING GEAR AND LINKAGE REMOVAL/INSTALLATION.)
5 | Stabilizer control link nut (lower)
6 | Front upper arm ball joint (See FRONT UPPER ARM REMOVAL/INSTALLATION.)
7 | Front upper arm bolt
8 | Front lower arm ball joint (See FRONT LOWER ARM REMOVAL/INSTALLATION.)
9 | Steering knuckle component
10 | Steering knuckle
11 | Dust cover
12 | Wheel hub bolt (See Wheel Hub Bolt Removal Note.) (See Wheel Hub Bolt Installation Note.)
13 | Wheel hub component

Brake Caliper Component Removal Note

1. Suspend the brake calliper component using a cable or equivalent.

amxzzw00001235

Wheel Hub Bolt Removal Note

  Note
  • Remove the dust cover only if there is an abnormality.

1. Remove the wheel hub bolts from the wheel hub using a press.

amxzzw00001236

Wheel Hub Bolt Installation Note

1. Press in new wheel hub bolts into the wheel hub using a press.

amxzzw00001237