TRUNK LID OPENER INSPECTION

id091400811400

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

3. Remove the trunk lid opener. (See TRUNK LID OPENER REMOVAL/INSTALLATION.)

4. Apply battery positive voltage and connect the ground to the corresponding the trunk lid opener terminals, and inspect the trunk lid opener operation.

amxzzw00002140

  • If the trunk lid opener does not operate as indicated in the table, replace the trunk lid opener.

Operation | Terminal
--- | ---
A | B
Unlocks | B+ | Ground