TRUNK LID OPENER SWITCH REMOVAL/INSTALLATION

id091400812200

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Using a small flathead screwdriver, detach the tabs of the trunk lid opener switch from the dashboard.

e5u914aw4011

3. Push the trunk lid opener switch into the dashboard and remove.

4. Disconnect the trunk lid opener switch connector.

5. Install in the reverse order of removal.