PROPELLER SHAFT INSPECTION

id031500800500

1. Use a dial gauge to measure the runout of the propeller shaft at each position.

amxzzw00002390

  • If it exceeds the maximum specification, replace the propeller shaft.

  Maximum runout

  0.6 mm {0.024 in}

2. Inspect the play and rotation of the joint by turning the universal joint in the direction shown by the arrow.

amxzzw00001312

  • If there is excessive play or initial torque, replace the propeller shaft.

  Initial torque (Reference value)

  0.29—0.98 N·m {3.0—10 kgf·cm, 2.7—8.6 in·lbf}