SIDE SHELF REMOVAL/INSTALLATION

id091700808200

Except Power Retractable Hardtop

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (8) Seat belt set plate (See SEAT BELT REMOVAL/INSTALLATION.)

  (9) Seat back crossmember assembly (See SEAT BACK CROSSMEMBER ASSEMBLY REMOVAL/INSTALLATION.)

  (10) Rear side trim (See REAR SIDE TRIM REMOVAL/INSTALLATION.)

  (11) Rear package trim (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

2. Remove the fasteners.

e5u917zw5033

3. Pull the side shelf outward and detach clip A.

4. Remove the side shelf.

5. Install in the reverse order of removal.

Power Retractable Hardtop

1. Fully open the deck panel.

2. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (8) Rear side trim (See REAR SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove the fasteners.

amxzzw00001422

4. Pull the side shelf outward and detach clip A.

5. Remove the side shelf.

6. Install in the reverse order of removal.