MAGNETIC CLUTCH ADJUSTMENT [MANUAL AIR CONDITIONER]

id0740a2800500

1. Measure the clearance around the entire circumference between the pressure plate and A/C compressor pulley using a thickness gauge.

e5u740zw5011

2. Inspect the clearance.

  • If not within the specification, adjust the clearance by changing the shim or the number of shims.

  Magnetic clutch clearance

  0.3—0.6 mm {0.012—0.023 in}