MAP LIGHT REMOVAL/INSTALLATION

id091800801200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Insert a tape-wrapped fastener remover into the service hole and pry with the fastener remover in the direction shown by the arrow to remove the lens.

amxzzw00002146

4. Remove the map light bulb

amxzzw00001027

5. Remove the map light. (See Map Light Removal Note.)

6. Disconnect the connector.

7. Install in the reverse order of removal.

Map Light Removal Note

1. Insert a tape-wrapped fastener remover into the gap between the front header trim and the map light.

2. Press the tab, and remove the map light.

amxzzw00001028