TWEETER/DOOR UPPER SPEAKER REMOVAL/INSTALLATION

id092000810900

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

4. Disconnect the connector.

amxzzw00002361

5. Remove the screws.

6. Remove the tweeter (without Bose®)/door upper speaker (with Bose®).

7. Install in the reverse order of removal.