CLUTCH PEDAL REMOVAL/INSTALLATION

id051000801200

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

amxzzw00002598

1 | Clutch switch connector
2 | Clutch switch
3 | Nut A (See Clip, Nut A and Nut B Installation Note.)
4 | Nut cap / Clip (See Nut Cap Removal Note.) (See Clip, Nut A and Nut B Installation Note.)
5 | Nut B (See Clip, Nut A and Nut B Installation Note.)
6 | Retaining ring
7 | Joint pin
8 | Bush
9 | Nut C
10 | Push rod
11 | Fork
12 | Pedal pad
13 | Clutch pedal component

Nut Cap Removal Note

1. Dispose of the nut cap after removal.

  Note
  • When installing the clutch pedal, install the clip instead of the nut cap.

Clip, Nut A and Nut B Installation Note

1. Temporarily tighten nut A.

amxzzw00002599

2. Insert the clip completely so that the clutch pedal adheres to the installation surface and there are no gaps between them.

3. Tighten the bolts B.

4. Tighten the bolt A completely.

5. After installing the clutch pedal component, inspect/adjust the clutch pedal. (See CLUTCH PEDAL ADJUSTMENT.)