FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

id091000800600

1. Disconnect the negative battery cable. (SeeBATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)

  (2) Front combination light (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

  (3) Fresh air duct (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)

  (4) Horn (See HORN REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

amxzzw00001497

1 | Clip
2 | Shroud seal plate
3 | Harness clip
4 | Front bumper reinforcement

4. Install in the reverse order of removal.