TRANSMISSION RANGE (TR) SWITCH INSPECTION [SJ6A-EL]

id051311251300

Operating inspection

1. Verify that the starter operates only when the ignition switch is turned to the START position with the selector lever in the P or N position.

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT [SJ6A-EL].)

2. Verify that the back-up lights illuminate when shifted to the R position with the ignition switch at the ON position.

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT [SJ6A-EL].)

3. Verify that the positions of the selector lever and the indicator are aligned.

L.H.D.

amxzzw00001103

R.H.D.

amxzzw00001104

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT [SJ6A-EL].)

Continuity Inspection

  Caution
  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the tunnel member component.

4. Remove the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

5. Remove the insulator.

e5u513zw5005

6. Disconnect the TR switch connector.

e5u513zw5006

7. Verify that the continuity is as indicated in the table.

amxzzw00000190

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT [SJ6A-EL].)

amxzzw00000181

8. Reinspect for continuity at TR switch.

  • If there is any malfunction, replace the TR switch. (See TRANSMISSION RANGE (TR) SWITCH REMOVAL/INSTALLATION [SJ6A-EL].)

9. Connect the TR switch connector.

10. Install the insulator.

  Tightening torque

  8—11 N·m {82—112 kgf·cm, 72—97 in·lbf}

11. Install the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

12. Install the tunnel member component.

13. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

14. Install the battery cover.