AUXILIARY JACK REMOVAL/INSTALLATION

id092000809900

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

5. Remove the console panel. (See CONSOLE PANEL REMOVAL/INSTALLATION.)

amxzzw00001685

6. While pressing the tabs, pull the auxiliary jack.

7. Install in the reverse order of removal.