MANUAL ANTENNA REMOVAL/INSTALLATION

id092000807300

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove in the order indicated in the table.

amxzzw00002299

1 | Antenna rod
2 | Mounting nut (See Mounting Nut Removal Note.)
3 | Spacer
4 | Connector
5 | Nut
6 | Manual antenna

4. Install in the reverse order of removal.

Mounting Nut Removal Note

1. Use snap‐ring pliers to remove the mounting nut.

e5u920zw5011