TRUNK LID ADJUSTMENT

id091000801700

1. Measure the gap and height difference between the trunk lid and the body.

2. Loosen the trunk lid hinge installation nuts or the trunk lid lock striker installation screws, and adjust the trunk lid.

e5u910zw1011

amxzzw00001905

  Standard clearance

  a: 4.5—7.5 mm {0.18—0.29 in} (Except Power Retractable Hardtop)
  a: 5.5—8.5 mm {0.22—0.33 in} (Power Retractable Hardtop)
  b: 5.0—9.0 mm {0.20—0.35 in}
  c: 3.0—6.0 mm {0.12—0.23 in} (Except Power Retractable Hardtop)
  c: 4.0—8.0 mm {0.16—0.31 in} (Power Retractable Hardtop)
  d: 3.0—5.0 mm {0.12—0.19 in}

3. Tighten the nuts. (See TRUNK LID REMOVAL/INSTALLATION)