ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION [DYNAMIC STABILITY CONTROL (DSC)]

id0402b2175200

• The PID/data monitor function is used for optionally selecting input/output signal monitor items preset in the DSC HU/CM and reading them out in real-time.

PID/DATA Monitor Table

PID/data monitor item | Input/output part | Unit/Condition (Tester display)
--- | --- | ---
ABS_VOLT | Battery | V
ABSLF_I | LF inlet solenoid valve | Off/On
ABSLF_O | LF outlet solenoid valve | Off/On
ABSLR_I | LR inlet solenoid valve | Off/On
ABSLR_O | LR outlet solenoid valve | Off/On
ABSPMPRLY | Pump motor relay | Off/On
ABSRF_I | RF inlet solenoid valve | Off/On
ABSRF_O | RF outlet solenoid valve | Off/On
ABSRR_I | RR inlet solenoid valve | Off/On
ABSRR_O | RR outlet solenoid valve | Off/On
ABSVLVRLY | Valve control relay | Off/On
BOO_ABS | Brake switch | Off/On
CCNTABS | Number of continuous DTCs | —
LAT_ACCL | Combined sensor (lateral-G value) | G
LF_WSPD | LF ABS wheel-speed sensor | KPH, MPH
LR_WSPD | LR ABS wheel-speed sensor | KPH, MPH
MCYLI P | Brake fluid pressure sensor | Pa, psi
PMP_MOTOR | Pump motor | Off/On
RF_WSPD | RF ABS wheel-speed sensor | KPH, MPH
RPM | PCM (engine speed) | RPM
RR_WSPD | RR ABS wheel-speed sensor | KPH, MPH
SWA_POS | Steering angle sensor | °
TPI | PCM (throttle opening angle) | %
V_STB_L | LH stability control solenoid valve | Off/On
V_STB_R | RH stability control solenoid valve | Off/On
V_TRC_L | LH traction control solenoid valve | Off/On
V_TRC_R | RH traction control solenoid valve | Off/On
YAW_RATE | Combined sensor (yaw rate value) | °/s