DRIVE BELT INSPECTION [L8, LF]

id0110a9801500

  Note
  • Drive belt deflection/tension inspection is not necessary because of the use of the auto tensioner.

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

  Note
  • Use a mirror to see the position of the drive belt auto tensioner indicator mark.

  e5u110zw5021

2. Verify that the drive belt auto tensioner indicator mark does not exceed the limit.

  • If it exceeds the limit, replace the drive belt. (See DRIVE BELT REPLACEMENT [L8, LF].)

AT

e5u110zw5020

MT

e5u110zw5001

3. Install the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)