DSC INDICATOR LIGHT OPERATION

id041500102300

• When the DSC and CAN lines are normal, the DSC indicator light illuminates for approx. 3 s when the ignition switch is turned to the ON position to check the light function. When the system is malfunctioning, the DSC indicator light remains illuminated.
• When the DSC or TCS is operating (DSC has not been disabled by pressing the DSC OFF switch), the DSC indicator light operates as follows:

DSC Indicator Light Operation

Item | DSC indicator light condition
TCS, DSC not operating | Not illuminated
TCS operating | Flashes (0.5 s intervals)
DSC operating
TCS, DSC system malfunction | Illuminated

amxzzn00000132