PID/DATA MONITOR TABLE [POWER RETRACTABLE HARDTOP]

id0902j2846000

PID/data monitor table

PID name (definition) | Unit/Operation | Operation Condition (Reference) | Terminal
--- | --- | --- | ---
DTC_CNT (Number of continuous DTCs) | – | • DTCs detected: 1—255 • No DTCs detected: 0 | –
VPWR (Module supply voltage) | V | Ignition switch is at ON: B+ | 1X
VSS (Vehicle speed) | KPH, MPH | • Vehicle stopped: 0 KPH {0 MPH} • Vehicle speed 25 km/h {16 mph}: 25 KPH {16 MPH} | –
RHT_OP (Power retractable hardtop limit switch (Open position)) | On/Off | • When power retractable hardtop is fully opened (Power retractable hardtop open position switch is on): On • Others (Power retractable hardtop open position switch is off): Off | 1T
RHT_CL (Power retractable hardtop limit switch (Close position)) | On/Off | • When power retractable hardtop is fully closed (Power retractable hardtop close position switch is on): On • Others (Power retractable hardtop close position switch is off): Off | 1R
DECK_OP (Deck panel limit switch (Open position)) | On/Off | • When deck panel is fully opened (Deck panel open position switch is on): On • Others (Deck panel open position switch is off): Off | 3F
DECK_CL (Deck panel limit switch (Close position)) | On/Off | • When deck panel is fully closed (Deck panel close position switch is off): On • Others (Deck panel close position switch is on): Off | 3O
SW_OP (Power retractable hardtop open switch) | On/Off | • When power retractable hardtop open switch is pressed: On • When power retractable hardtop open switch is released: Off | 1H
SW_CL (Power retractable hardtop close switch) | On/Off | • When power retractable hardtop close switch is pressed: On • When power retractable hardtop close switch is released: Off | 1H
SW_STRIKER (Top lock switch) | On/Off | • When top lock is locked: On • When top lock is unlocked: Off | 1D
SW_TRUNK (Trunk lid opener switch) | On/Off | • Trunk lid is open: Off • Trunk lid is closed: On | 1F
TR_OP_CTL (Trunk opener control) | On/Off | • Power retractable hardtop operating (Trunk lid open operation is disabled): On • Power retractable hardtop not operated (Trunk lid open operation is enabled): Off | –
Indicator (Power retractable hardtop indicator light) | On/Off | • When power retractable hardtop indicator light is illuminated: On • When power retractable hardtop indicator light is turned off: Off | 2C