POWER RETRACTABLE HARDTOP CONTROL MODULE BRACKET REMOVAL/INSTALLATION

id091600809500

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

4. Remove the roof hook cable case.

amxzzw00002074

5. Remove in the order indicated in the table.

amxzzw00002075

1 | Connector
2 | Nut
3 | Bolt
4 | Power retractable hardtop control module assembly

6. Remove the nuts.

amxzzw00002076

7. Remove the power retractable hardtop control module from the power retractable hardtop control module bracket.

8. Install in the reverse order of removal.