PID/DATA MONITOR TABLE [AIR BAG SYSTEM]

id0802a0800800

PID/data monitor table

PID name (definition) | Unit/Condition | Operation Condition (Reference) | Terminal
--- | --- | --- | ---
CCNT_RCM (Number of continuous DTCs) | — | • DTCs detected: 1—255 • No DTCs detected: 0 | —
CR2D_Comm (Driver-side side air bag sensor system communication data error) | OK/ FAULT | • Sensor normal: OK • Sensor communication malfunction: FAULT | 2C, 2F
CR2D_Inter (Driver-side side air bag sensor system internal circuit disabled) | OK/ FAULT | • Sensor normal: OK • Sensor internal malfunction: FAULT | 2C, 2F
CR2D_Mount (Driver-side side air bag sensor assembly incorrect) | OK/ FAULT | • Sensor normal: OK • Sensor Install malfunction: FAULT | 2C, 2F
CR2D_Short (Driver-side side air bag sensor system communication error) | OK/ FAULT | • Sensor normal: OK • Sensor open or short circuit: FAULT | 2C, 2F
CR2P_Comm (Passenger-side side air bag sensor system communication data error) | OK/ FAULT | • Sensor normal: OK • Sensor communication malfunction: FAULT | 2X, 2AA
CR2P_Inter (Passenger-side side air bag sensor system internal circuit disabled) | OK/ FAULT | • Sensor normal: OK • Sensor internal malfunction: FAULT | 2X, 2AA
CR2P_Mount (Passenger-side side air bag sensor assembly incorrect) | OK/ FAULT | • Sensor normal: OK • Sensor Install malfunction: FAULT | 2X, 2AA
CR2P_Short (Passenger-side side air bag sensor system communication error) | OK/ FAULT | • Sensor normal: OK • Sensor open or short circuit: FAULT | 2X, 2AA
IGN_V_2 (IG1 voltage) | V | Ignition switch is at ON: B+ | —
I_PAD_SW (PAD switch status) | On/ Off | • PAD switch is at PASS AIRBAG ON position: On • PAD switch is at PASS AIRBAG OFF position: Off | —
RES_AB_D (Driver-side air bag module resistance) | ohm | Under any condition: 1.5—4.7 ohms | 1A, 1D
RES_AB_P (Passenger-side air bag module resistance) | ohm | Under any condition: 1.3—4.7 ohms | 1S, 1V
RES_PT_D (Driver-side pre-tensioner seat belt resistance) | ohm | Under any condition: 1.3—4.7 ohms | 2A, 2D
RES_PT_P (Passenger-side pre-tensioner seat belt resistance) | ohm | Under any condition: 1.3—4.7 ohms | 2V, 2Y
RES_SAB_D (Driver-side side air bag module resistance) | ohm | Under any condition: 1.3—4.7 ohms | 2G, 2J
RES_SAB_P (Passenger-side side air bag module resistance) | ohm | Under any condition: 1.3—4.7 ohms | 2P, 2S