AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

id0740a1801600

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

L.H.D.

e5u740zw5005

R.H.D.

amxzzw00000976

1 | Airflow mode actuator connector
2 | Airflow mode actuator

5. Install in the reverse order of removal.