WIPER MOTOR REMOVAL/INSTALLATION

id091900804500

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the wiper arm and blade. (See WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

4. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

5. Disconnect the connector.

amxzzw00000740

6. Remove the bolts.

7. Remove the nut.

8. Install in the reverse order of removal.